KNX S4-B12 24 V actuator invitation to tender

Actuator for the KNX bus system. 4 outputs, 1 for each drive (up/down) with polarity change for motor 12 V DC / 24 V DC. 12 binary inputs (actuator or bus keys) with variable voltage 6...24 V DC. Drive runtime measurement (position feedback). Storage of a movement position, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or exhaust air level control, blocks, locks and priority stipulations. 
585 communication objects.
Rail-mounted device (6 division units) with 4 key pairs and status LEDs. Dimensions 107 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70533 KNX S4-B12 24 V