Actuator KNX DALI L4 bc 16 A

Actuator as interface between KNX bus system and DALI lighting system. 4 channels. Per channel 
•	one DALI control output for up to 64 participants ( EVGs ) via broadcast telegram. (18 V typical, max. 128 mA).
•	A relay contact to interrupt the power supply to the participants (standby avoidance). 230 V AC, 16 A, 165 A/20 ms, 490 A/1.5 ms (electronic ballast).
•	On/Off buttons on the unit for commissioning. Switching and dimming without bus voltage.
•	Status LEDs for relay and luminaire.
Functions: Normal operation, night operation, staircase timer with adjustable prewarning, night operation with staircase timer. Colour temperature control (Tunable White), RGB/RGBW colour control, HSV colour control, scene calls, status feedback, time functions.
Delivers DALI bus voltage, no external supply required. Operating voltage 230 V AC, 50 Hz. Inrush current limitation by time-delayed switching of the channels with simultaneous switch-on command. 

165 communication objects.
Mounting: Rail-mounted device 
Dimensions: approx. 107 x 88 x 60 (W x H x D, mm), 6 division units

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70580 KNX DALI L4 bc 16 A