Cala KNX M1-T push button, pure white RAL 9010

1-gang push button with temperature sensor for the KNX bus system. With 1 touch button (bus push button) and 1 configurable LED (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 44 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70860 Cala KNX M1-T, pure white RAL 9010

Cala KNX M1-T push button, jet black RAL 9005

1-gang push button with temperature sensor for the KNX bus system. With 1 touch button (bus push button) and 1 configurable LED (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 44 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70862 Cala KNX M1-T, jet black RAL 9005

Cala KNX M2-T push button, pure white RAL 9010

2-gang push button with temperature sensor for the KNX bus system. With 2 touch buttons (bus push buttons) and 2 configurable LEDs (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 55 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70870 Cala KNX M2-T, pure white RAL 9010

Cala KNX M2-T push button, jet black RAL 9005

2-gang push button with temperature sensor for the KNX bus system. With 2 touch buttons (bus push buttons) and 2 configurable LEDs (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 55 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70872 Cala KNX M2-T, jet black RAL 9005

Cala KNX M4-T push button, pure white RAL 9010

4-gang push button with temperature sensor for the KNX bus system. With 4 touch buttons (bus push buttons) and 4 configurable LEDs (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 73 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70880 Cala KNX M4-T, pure white RAL 9010

Cala KNX M4-T push button, jet black RAL 9005

4-gang push button with temperature sensor for the KNX bus system. With 4 touch buttons (bus push buttons) and 4 configurable LEDs (switching via objects).
Application program with temperature mixed value calculation, 2 AND logic gates und 2 OR logic gates. 73 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70882 Cala KNX M4-T, jet black RAL 9005