Cala KNX MultiTouch T Light/Sunblind push button, pure white RAL 9010

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	Drive (up/down with distinction short/long, driving position)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 199 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70890 Cala KNX MultiTouch T Light/Sunblind, pure white RAL 9010

Cala KNX MultiTouch T Light/Sunblind push button, jet black RAL 9005

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	Drive (up/down with distinction short/long, driving position)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 199 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70892 Cala KNX MultiTouch T Light/Sunblind, jet black RAL 9005

Cala KNX MultiTouch T Light/Scenes push button, pure white RAL 9010

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	3 scenes (recall and storage)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 198 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70960 Cala KNX MultiTouch T Light/ Scenes, pure white RAL 9010

Cala KNX MultiTouch T Light/Scenes push button, jet black RAL 9005

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	3 scenes (recall and storage)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 198 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70960 Cala KNX MultiTouch T Light/ Scenes, jet black RAL 9005

Cala KNX MultiTouch T Light push button, pure white RAL 9010

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 199 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: pure white RAL 9010.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70950 Cala KNX MultiTouch T Light, pure white RAL 9010

Cala KNX MultiTouch T Light push button, jet black RAL 9005

Push button with temperature sensor for the KNX bus system. With 9 configurable touch buttons (bus push buttons), divided into 3 areas, printed with icons for the functions:
•	Light (switching and dimming) with configurable LED (switching via objects)
•	Temperature control (warmer, cooler, changeover heating/cooling) with configurable LEDs (switch via objects). 
Area function when several push buttons are touched.
Application program with temperature mixed value calculation, 4 AND logic gates und 4 OR logic gates. Scene control. PI controller for heating/cooling (by temperature). 199 communication objects. 
Glass surface. Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W x H in mm), installation depth approx. 10 mm, Base plate dimensions: approx. 71 x 71 (W x H in mm). Operating voltage: KNX bus voltage.
Colour: jet black RAL 9005.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70952 Cala KNX MultiTouch T Light, jet black RAL 9005